# ACS221 –Control System Design Assignment

## Question 1

**A unity feedback servo system has a plant with the transfer function given by:**

**Question A: Using the frequency domain approach, determine the gain K required to give an  
overshoot, in response to a step input, of approximately 20%. Explain how you  
achieved your result.**

**The plant is a third order system which has 82.86% overshoot with unity feedback, and the target is lower the overshoot to 20%.**

**To get the 20% overshoot, the following equation is used during the calculation, the maximum overshoot can be obtained by using to get** and then work out the phase margin using the equation below that, and use the bode diagram to find out the gain crossover frequency for that phase margin. Then use the property of the |K\*G(jw)|= 0dB=1, plug in the w inside the equation to work out the K. And the K is required proportional gain compensator.




In practical, the  **is considered a bit lower than the requirement, in this case, it was set to 14% overshoot, which is 0.14 in equivalent of ,**



And the phase margin will be:




Therefore the gain crossover frequency is located at phase angle -180+48.73, which is -131.27. The plot is shown below



Figure

By Converting dB to gain, which 27.4dB =10^(27.4/20)=23.44, the K is 1/|G(jw)|, which is 0.043, and the closed loop response with this K is shown in figure.2



Figure

The peak overshoot with K=0.043 is 18.5%. It is close to required 20% with less than 10% error.

**B. Using frequency domain approach, design a lead compensator to achieve a  
velocity error constant that is at least 35 and a step response overshoot that is  
no greater than 20%. Describe each stage of your design. If performance  
specifications are not met first time, perform additional design iterations (i.e.  
refine the lead compensator or design additional compensators/pre-filter).  
Write down the final compensated open- and closed-loop transfer functions and  
use MATLAB to evaluate the performance of your final design in the time and  
frequency domain.  
Use MATLAB to plot the response of the control system to a unit ramp, showing  
both system output and ramp input, and evaluate the percentage steady state  
error to the ramp input signal.  
Summarize the performance indices of your final design in a table – see Table 1 -  
and provide a written conclusion for your design.**

First, the k can be calculated by using Kv given in the question and the Kv is 35

K=4.62

The feedback of the plant is G\*k

The peak overshoot can be satisfied by finding from equation,




And the phase margin is 


The plant currently has -4.82 degree phase margin, which means another 52.97 degree of phase margin

To find alpha, the equation used in the calculation is

And the α is 11.11

However, when implanting lead compensator, the gain and phase margin increases, so we need to find new gain crossover frequency to compensate new added gain.





However, with this lead compensator, the new plant has only 27.3 phase margin which is around half of the desired phase margin. To solve this issue, another lead compensator is required.